;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
;
; .dat file for the display driver component dll
;
; Abstract:
; The Key value will overwrite the dll code and will be returned by the component dll.
; Therefore, the key value should not be defined if the value is expected from the dll code.
; The dat file (if used) should have the same prefix name of the dll file.
; 
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;

[Component]

Name=FIRE GL driver for 3D Studio MAX/VIZ 

;Traditional Chinese
Name_cht=FIRE GL driver for 3D Studio MAX/VIZ
;Simplified Chinese
Name_chs=FIRE GL driver for 3D Studio MAX/VIZ
;Danish
Name_dan=FIRE GL driver for 3D Studio MAX/VIZ
;Dutch
Name_nld=FIRE GL driver for 3D Studio MAX/VIZ
;English
Name_enu=FIRE GL driver for 3D Studio MAX/VIZ
;Finnish
Name_fin=FIRE GL driver for 3D Studio MAX/VIZ
;French
Name_fra=FIRE GL driver for 3D Studio MAX/VIZ
;German
Name_deu=FIRE GL Treiber f黵 3D Studio MAX/VIZ

;Italian
Name_ita=FIRE GL driver for 3D Studio MAX/VIZ
;Japanese
Name_jpn=FIRE GL driver for 3D Studio MAX/VIZ
;Korean
Name_kor=FIRE GL driver for 3D Studio MAX/VIZ
;Norwegian
Name_nor=FIRE GL driver for 3D Studio MAX/VIZ

;Spanish
Name_esp=FIRE GL driver for 3D Studio MAX/VIZ
;Swedish
Name_sve=FIRE GL driver for 3D Studio MAX/VIZ

;Default
Description=Install FIRE GL driver for 3D Studio MAX/VIZ

;Traditional Chinese
Description_cht=杆3D Studio MAX/VIZFIRE GL臱笆祘Α
;Simplified Chinese
Description_chs=安装3D Studio MAX/VIZ的FIRE GL驱动程序

;Danish
Description_dan=Installation af FIRE GL-driverne for 3D Studio MAX/VIZ
;Dutch
Description_nld=Installatie van het FIRE GL stuurprogramma voor 3D Studio MAX/VIZ
;English
Description_enu=Install FIRE GL driver for 3D Studio MAX/VIZ
;Finnish
Description_fin=Asenna FIRE GL ajuri 3D Studio MAX/VIZ varten
;French
Description_fra=Installer le pilote FIRE GL pour Studio MAX/VIZ 3D
;German
Description_deu=Installation der FIRE GL-Treiber f黵 3D Studio MAX/VIZ

;Italian
Description_ita=Installazione driver FIRE GL per 3D Studio MAX/VIZ
;Japanese
Description_jpn=3D Studio MAX/VIZ 梡偵 FIRE GL 僪儔僀僶傪僀儞僗僩乕儖
;Korean
Description_kor=3D 胶譬叼坷 MAX/VIZ甫 困茄 FIRE GL-靛扼捞滚狼 汲摹
;Norwegian
Description_nor=Installasjon av FIRE GL-driveren for 3D studio MAX/VIZ

;Spanish
Description_esp=Instale el controlador FIRE GL para 3D Studio MAX/VIZ
;Swedish
Description_sve=Installation av  FIRE GL drivrutiner f鰎 3D Studio MAX/VIZ


; cds defines the path of the Component Detection Service
CDS=..\bin

;
; Req_ASIC=<Device id 1>,<Device id 2>, ...
; Gives the PCI device ID to check for requirement. 
; If the FGL ASIC is found, then MeetsRequirement from the dll will return 1.
; If the last 2 digits are 00, it means the last 2 digits are "don't care"
; For example, R128 family - 5200; Rage PRO family - 4700
;              Rage PRO (GB) - 4742
;;;HN;;;Req_ASIC=514C,514E,514F,4242,5144,4C57,4C58,4C59,5157,5159,4336,4136,516C,4137,4337

;
; !Req_ASIC=<Device id 1>,<Device id 2>, ...
; Gives the PCI device ID to check for requirement. 
; If the FGL ASIC is found, then MeetsRequirement from the dll will return 0.
; If the last 2 digits are 00, it means the last 2 digits are "don't care"
; For example, R128 family - 5200; Rage PRO family - 4700
;              Rage PRO (GB) - 4742
;!Req_ASIC=4700

;
; Req_Capture=<Vendor id Device id 1>,<Vendor id Device id 2>, ...
; Gives the PCI vendor and device ID to check for requirement. 
; If the Capture ASIC is found, then MeetsRequirement from the dll will return 1.
; If the last 2 digits are 00, it means the last 2 digits are "don't care"
; For example, BT878 - 109e0878 (where 109e is the vendor id, 878 is the device id)
;Req_Capture=109e0878

;
; !Req_Capture=<Vendor id Device id 1>,<Vendor id Device id 2>, ...
; Gives the PCI vendor and device ID to check for requirement. 
; If the Capture ASIC is found, then MeetsRequirement from the dll will return 0.
; If the last 2 digits are 00, it means the last 2 digits are "don't care"
; For example, BT878 - 109e0878 (where 109e is the vendor id, 878 is the device id)
;!Req_Capture=109e0878

;
; Req_Tuner=1,NTSC,PAL,SECAM,SCART,0
; Check if the Tuner attached has the standard required, the MeetsRequirement will return 1
;
;Req_Tuner=PAL,SECAM

CheckFGL=1

; 0=no, 1=yes
;MeetsRequirement=0

; in KB         
Size=150

; 0, 1, 2 ... where 0 is the highest order
Order=2

; 0=no, 1=yes
;Reboot=0

; OS can be 1, WIN_95, WIN_95_OSR2_USB, WIN_98, WIN_NT351, WIN_NT4, WIN_NT5, WIN_98_GOLD
; WIN_98_SE, WIN_ME
OS=WIN_2K, WIN_XP

; 0=no, 1=yes
;Visible=0                  

; 0=no, 1=yes
;WaitMessage=0               

; <Comp#1>,<Comp#2>
;ReqComp=DirectX
ReqComp=DRIVER

; For display driver, we have to launch silent child install.
InstallCommandLine=setup.exe,/K

;Component Version
Ver=6.14.10.5005

;Requires Uninstall before installing this component
;UninstallComp=FGL Display Driver,FGL Video Player
